9. Raspberry Pi code :-

import RPi.GPI0 as GPI0

import time

GPI0.setmode(GPI0.BOARD)

while True:

GPI0.setup(3.GPI0.OUT)

GPI0.output(3.True)

time.sleep(0.5):

GPI0.output(3.False)

time.sleep(0.5)